PT SAPTA BORNEO UTAMA
Institutional Virtual Data Room
SBU-TEC-001 Confidential Final / Published

# Technical Design Basis

Technical design criteria and engineering assumptions supporting the 10,000 TCD Sugar Mill, 60 KLPD Ethanol Plant and 30 MW Biomass Power Plant.

## Project Configuration

Component | Capacity
--- | ---
Sugar Mill | 10,000 TCD
Ethanol Plant | 60 KLPD
Biomass Power Plant | 30 MW
Core Plantation | 500 Ha
Expansion Program | 10,000–20,000 Ha

## Design Principles

- High-efficiency sugar extraction process
- Integrated ethanol production from molasses
- Bagasse-based cogeneration system
- Scalable industrial layout
- Environmental compliance and ESG integration

## Engineering Standards

- International EPC standards
- Applicable Indonesian regulations
- Industrial safety and fire protection standards
- Environmental management requirements
- Project finance lender technical requirements